This chapter documents the backend for the 8080/z80/gbz80/64180/RCMx000
microprocessor family.

@section Legal

    This module is copyright in 2009 by Dominic Morris

@section Additional options for this module

This module provides the following additional options:

@table @option
    @item -8080
        Turns on 8080 compatibility mode. Any use of z80 (or higher)
        opcodes will result in an error being generated.
    @item -gbz80
        Turns on gbz80 compatibility mode. Any use of non-supported
        opcodes will result in an error being generated.
    @item -hd64180
        Turns on 64180 mode supporting additional 64180 opcodes.
    @item -rcm2000
    @item -rcm3000
    @item -rcm4000
         Turns on Rabbit compatibility mode, generating the correct
         codes for moved opcodes and supporting the additional Rabbit
         instructions. In this mode, 8 bit access to the 16 bit index
         registers is not permitted.
    @item -rcmemu
         Turns on emulation of some instructions which aren't available
         on the Rabbit processors.
    @item -swapixiy
        Swaps the usage of ix and iy registers. This is useful
        for compiling generic code that uses an index register that
        is reserved on the target machine.
    @item -z80asm
         Switches on z80asm mode. This translates ASMPC to $ and accepts
         some pseudo opcodes that z80asm supports. Most emulation of 
         z80asm directives is provided by the oldsyntax syntax module.         
@end table

@section General

This backend accepts z80 family instructions in standard
Zilog syntax. Rabbit opcodes are accepted as defined in the 
publically available reference material from Rabbit Semiconductor,
with the exception that the @code{ljp} and @code{lcall} opcodes need
to be supplied with a 24 bit number rather than an 8 bit @code{xpc} and a
16 bit address.

The target address type is 16 bit.

Instructions consist of one up to six bytes and require no alignment.
There is also no alignment requirement for sections and data.

@section Extensions

This backend provides the following specific extensions:

@itemize @minus

@item Certain Rabbit opcodes can be prefixed by the @code{altd} and/or the
 @code{ioi}/@code{ioe} modifier.
 For details of which instructions these are valid for please
 see the documentation from Rabbit.

@item The parser understands a lo/hi-modifier to select low- or high-byte
 of a 16-bit word. The character @code{<} is used to select the low-byte
 and @code{>} for the high-byte. It has to be the first character before
 an expression.

@item When applying the operation @code{/256}, @code{%256} or @code{&256}
 on a label, an appropriate lo/hi-byte relocation will automatically be
 generated.

@end itemize

@section Optimisations

This backend supports the emulation of certain z80 instructions on the
Rabbit/gbz80 processor. These instructions are @code{rld}, @code{rrd},
@code{cpi}, @code{cpir}, @code{cpd} and @code{cpdr}.
The link stage should provide routines with the opcode name prefixed with
@code{rcmx_} (eg @code{rcmx_rld}) which implements the same functionality.
Example implementations are available within the z88dk CVS tree.

Additionally, for the Rabbit targets the missing call @code{cc}, opcodes
will be emulated.

@section Known Problems

    Some known problems of this module at the moment:

@itemize @minus

@item Not all RCM4000 opcodes are supported (@code{llcall}, @code{lljp}
 are not available).

@end itemize

@section Error Messages

This module has the following error messages:

@itemize @minus
@item 2001: index offset out of bounds (%d)
@item 2002: Opcode not supported by %s (%s)
@item 2003: Index registers not available on 8080
@item 2004: out of range for 8 bit expression (%d)
@item 2005: invalid bit number (%d) should be in range 0..7
@item 2006: rst value out of range (%d/0x%02x)  
@item 2007: %s value out of range (%d)
@item 2008: index offset should be a constant
@item 2009: invalid branch type for jr
@item 2010: Rabbit target doesn't support rst %d
@item 2011: Rabbit target doesn't support 8 bit index registers 
@item 2012: z180 target doesn't support 8 bit index registers
@item 2013: invalid branch type for jre
@item 2014: Opcode not supported by %s (%s) but it can be emulated (-rcmemu)
@item 2015: %s specifier is only valid for Rabbit processors
@item 2016: Only one of ioi and ioe can be specified at a time
@item 2017: %s specifier is not valid for the opcode %s
@item 2018: %s specifier redundant for the opcode %s
@item 2019: %s specifier has no effect on the opcode %s
@item 2020: Operand value must evaluate to a constant for opcode %s
@item 2021: Unhandled operand type wanted 0x%x got 0x%x
@item 2022: Missed matched index registers on %s
@item 2023: Only out (c),0 is supported for the opcode %s
@item 2024: Operations between different index registers are forbidden
@item 2025: Operations between ix/iy/hl are forbidden
@item 2026: Double indirection forbidden
@end itemize
